Basic Information： Standard PCB

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
| Product No. : | W535868AS2P3 | Order Status : | Pass, Payment |
| Create Time : | 2023/3/28 20:42:16 | Build Time : | 24hours |
| Estimated Finish Time : | 2023-03-30  China Time Zone(GMT+8) | Gerber File : | [openx65-mobo-rev01b-grb.zip](https://pcbwayfile.s3.us-west-2.amazonaws.com/gerber/23/03/28/2042251171463.zip?X-Amz-Expires=3600&response-content-disposition=attachment%3B%20filename%20%3D%22W535868AS2P3_openx65-mobo-rev01b-grb.zip%22&X-Amz-Algorithm=AWS4-HMAC-SHA256&X-Amz-Credential=AKIAJYTP4ACVZIZRAH7A/20230328/us-west-2/s3/aws4_request&X-Amz-Date=20230328T151129Z&X-Amz-SignedHeaders=host&X-Amz-Signature=5e8727405eaf04dbeba2dab7b106b5be754e0567a5158f57faffe6621d24174a) |

Parameter Information :

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
| Board type : | Single pieces | Panel Way : |  |
| Different Design in Panel： | 1 | X-out Allowance in Panel : |  |
| Size : | 100 x 100 mm | Quantity : | 5 |
| Layer : | 2 Layers | Material : | FR-4: TG150 |
| Thickness : | 1.6 mm | Min Track/Spacing : | 5/5mil |
| Min Hole Size : | 0.3mm ↑ | Solder Mask : | Green |
| Silkscreen : | White | Edge connector : | No |
| Surface Finish : | HASL with lead | "HASL" to "ENIG" | No |
| Via Process : | Tenting vias | Finished Copper : | 1 oz Cu |
| Remove pcb identification number : |  | Additional Options : | UL Marking:None, |
| Date Code : | None |  |  |
| PO No. : |  | Manufacturing : |  |
| Total: **US $5.00** | | | |